## /

## /wifi

Acccess Point 01
Acccess Point 02
Acccess Point 03
Acccess Point 04
Acccess Point 05
Acccess Point 06
Acccess Point 07
Acccess Point 08
Acccess Point 09
Acccess Point 10
100%
Acccess Point 11
70%
Acccess Point 12
10%
Acccess Point 13
100%
Acccess Point 14
66%
Acccess Point 15
56%
{v}
SSID
Password

### custom parameter

Label for Custom Param
{p}

#### Saving Credentials

Trying to connect ESP to network.
If it fails reconnect to AP to try again
Connected to {v}
with IP {i}
Not Connected to {v}{r}
Not Connected to apname
Authentication Failure
AP not found
Could not Connect
No AP set

#### H4 Color Header P

content

#### H4 Color Header S

content

## /info

Chip ID
  123456
Flash Chip ID
  1234556
IDE Flash Size
  4194304 bytes
Real Flash Size
  4194304 bytes
Empty
Soft AP IP
  192.168.4.1
Soft AP MAC
  00:00:00:00:00:00
Station MAC
  00:00:00:00:00:00

### Available Pages

Page | Function
--- | ---
/ | Menu page.
/wifi | Show WiFi scan results and enter WiFi configuration.(/0wifi noscan)
/wifisave | Save WiFi configuration information and configure device. Needs variables supplied.
/close | Close the configuration server and configuration WiFi network.
/info | Information page
/close | Close the captiveportal popup,configportal will remain active
/exit | Exit Config Portal, configportal will close
/restart | Reboot the device
/erase | Erase WiFi configuration and reboot Device. Device will not reconnect to a network until new WiFi configuration data is entered.

More information about WiFiManager at https://github.com/tzapu/WiFiManager
Form UPLOAD
* Upload may not function inside captive portal, Open in browser - http://192.168.4.1

Label for Custom Param
Choice1
Choice2